IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Mineral_Point_Residence.ifc"
Time stamp: "2023-08-09T16:20:42-05:00"
Preprocessor: "IfcOpenShell v0.7.0-fc50bdd3a"
Originating system: "BlenderBIM 0.0.230706"
Authorization: "Nobody"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  40 x Person "ryan@openingdesign.com" of Organization (no name given)
  32 x Organization "Autodesk Revit 2020 (ENU)"
  4 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1680878644 (2023-04-07T14:44:04Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1661457979 (2022-08-25T20:06:19Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682123705 (2023-04-22T00:35:05Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1633996150 (2021-10-11T23:49:10Z)
  31 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682305051 (2023-04-24T02:57:31Z)
  2 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1681941947 (2023-04-19T22:05:47Z)

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: square foot (conversion based)
  LENGTHUNIT: foot (conversion based)
  VOLUMEUNIT: cubic foot (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      contains 220 elements
        15 x IFCWALL | type IFCWALLTYPE "M358BØD_EX" | names: "Wall" | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing
        18 x IFCWINDOW | type IFCWINDOWTYPE "Empty" | names: "Window" | material: profiles "existing" ("WINDOW") | property sets: EPset_Parametric, EPset_Drawing, Pset_WindowCommon
        3 x IFCPLATE | type IFCPLATETYPE "Empty" | names: "Plate" | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301) | property sets: EPset_Parametric, EPset_Drawing, Pset_PlateCommon
        1 x IFCDOOR | type IFCDOORTYPE "3070L-SF" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, EPset_Drawing, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "3070R-SF" | SINGLE_SWING_RIGHT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "21070R" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        2 x IFCDOOR | type IFCDOORTYPE "21070R" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Neufert Toilet with Cistern" | BATH | names: "Furniture.001" | property sets: Pset_SanitaryTerminalTypeCommon
        1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Generic Medium Sink" | BATH | names: "Furniture.002" | property sets: EPset_Drawing, Pset_SanitaryTerminalTypeCommon
        1 x IFCDOOR | type IFCDOORTYPE "21070L" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon
        1 x IFCDOOR | type IFCDOORTYPE "34"84"L" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "21070L" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "3070R" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCDOOR | type IFCDOORTYPE "36"84"R" | SINGLE_SWING_LEFT | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        1 x IFCFURNITURE | BED | names: "Plane" | material: constituents "existing" () | property sets: EPset_Drawing, Pset_FurnitureTypeCommon
        5 x IFCFURNITURE | names: "Cube", "Plane", "Plane.001" (+2 more) | material: "CASEWORK" | property sets: Pset_FurnitureTypeCommon, EPset_Drawing
        1 x IFCSANITARYTERMINAL | type IFCFURNITURETYPE "Neufert Medium Basin" | BATH | names: "Furniture" | property sets: Pset_SanitaryTerminalTypeCommon
        1 x IFCDOOR | type IFCDOORTYPE "3070L-SF" | names: "Door" | material: "DOOR" | property sets: Pset_DoorCommon, Qto_DoorBaseQuantities
        2 x IFCWALL | type IFCWALLTYPE "M6BØD" | names: "Wall" | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
        5 x IFCWALL | type IFCWALLTYPE "M358BØD_DEMO" | names: "Wall" | material: layers "demolish" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, EPset_Drawing, Pset_WallCommon, Qto_WallBaseQuantities
        1 x IFCWALL | type IFCWALLTYPE "W2" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
        1 x IFCWALL | type IFCWALLTYPE "W1" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
        3 x IFCWALL | type IFCWALLTYPE "EX" | names: "Wall" | material: layers "existing" ("b" 0.416667014360428, "WINDOW" 0.416667014360428) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing
        1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "ADA Grab Bars" | names: "SanitaryTerminal" | property sets: Pset_SanitaryTerminalTypeCommon
        1 x IFCWINDOW | type IFCPLATETYPE "Empty" | LIGHTDOME | names: "Plate" | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301) | property sets: EPset_Parametric, EPset_Drawing, Pset_WindowCommon
        2 x IFCDOOR | type IFCDOORTYPE "36"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: OD_Options, Pset_DoorCommon
        1 x IFCDOOR | type IFCDOORTYPE "36"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: OD_Options, Pset_DoorCommon
        5 x IFCSLAB | type IFCSLABTYPE "NEW ASPHALT DRIVE WAY" | names: "Slab" | material: layers "20Fill" ("ASPHALT DRIVEWAY" 0.984251976013184) | property sets: EPset_Parametric, EPset_Drawing, OD_Options, Pset_SlabCommon
        1 x IFCDOOR | type IFCDOORTYPE "30"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
        7 x IFCSLAB | type IFCSLABTYPE "COMPOSITE DECK - HORZ." | names: "Slab" | material: layers "HorzLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric, OD_Options, EPset_Drawing, Pset_SlabCommon
        9 x IFCSLAB | type IFCSLABTYPE "COMPOSITE DECK - VERT." | names: "Slab" | material: layers "VertLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric, OD_Options, Pset_SlabCommon, Qto_SlabBaseQuantities, EPset_Drawing
        2 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Neufert Washing Machine" | names: "ElectricAppliance" | property sets: OD_Options, Pset_ElectricApplianceTypeCommon
        2 x IFCSANITARYTERMINAL | BATH | names: "Cube" | property sets: OD_Options, Pset_SanitaryTerminalTypeCommon
        2 x IFCSLAB | type IFCSLABTYPE "CONCRETE SLAB" | names: "Slab" | material: layers "concrete" ("CONCRETE RAMP & LANDING" 0.5) | property sets: EPset_Parametric, OD_Options, Pset_SlabCommon, EPset_Drawing
        2 x IFCSLAB | BASESLAB | names: "Cube" | property sets: OD_Options, Pset_SlabCommon
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | names: "SanitaryTerminal" | property sets: OD_Options, Pset_SanitaryTerminalTypeCommon
        21 x IFCBUILDINGELEMENTPROXY | names: "Cube", "Trace" | property sets: OD_Options, Pset_BuildingElementProxyCommon, EPset_Drawing
        9 x IFCWALL | type IFCWALLTYPE "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, OD_Options, EPset_Drawing
        1 x IFCDOOR | type IFCDOORTYPE "24"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: OD_Options
        2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Sink 124x44" | names: "SanitaryTerminal" | property sets: EPset_Drawing, OD_Options, Pset_SanitaryTerminalTypeCommon
        1 x IFCWALL | type IFCWALLTYPE "GENERIC 7"" | names: "Wall" | material: layers "poche" ("GENERIC POCHE" 0.583333313465118) | property sets: EPset_Parametric, OD_Options
        1 x IFCRAILING | GUARDRAIL | names: "Vert" | property sets: OD_Options, Pset_RailingCommon, EPset_Drawing
        10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Core_Fill_8in" | names: "BuildingElementProxy" | property sets: BBIM_Array
        1 x IFCFURNITURE | object type "BENCH" | USERDEFINED | names: "Plane" | material: "BENCH - COMPOSITE DECKING" | property sets: OD_Options, Pset_FurnitureTypeCommon
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Horz Ladder Reinforcing" | names: "BuildingElementProxy" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)"
        10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "8inCMU" | names: "BuildingElementProxy" | property sets: BBIM_Array
        1 x IFCSLAB | type IFCSLABTYPE "EXISTING DRIVEWAY" | names: "Slab" | material: layers "10Fill" ("EXISTING ASPHALT DRIVEWAY" 0.984251976013184) | property sets: EPset_Parametric, EPset_Drawing, OD_Options
        2 x IFCSLAB | type IFCSLABTYPE "FLR150" | names: "Slab" | material: layers ("GENERIC_FLOOR" 1.) | property sets: EPset_Parametric, Pset_SlabCommon
        11 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Morter_8inCMU" | names: "BuildingElementProxy" | property sets: BBIM_Array
        1 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Retail 8-Seater Rectangular Table" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
        1 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Retail 6-Seater Circular Table" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon, EPset_Drawing
        10 x IFCWALL | ELEMENTEDWALL | names: "A-Wall_curve_.001", "A-Wall_curve_", "A-Mill_curve_" (+7 more) | property sets: Pset_WallCommon, EPset_Drawing, Pset_FurnitureTypeCommon, OD_Options, Pset_DoorCommon, Pset_SanitaryTerminalTypeCommon
        3 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "A-Above_curve_", "A-Below_curve_", "A-Dims_curve_" | property sets: Pset_BuildingElementProxyCommon
        2 x IFCSANITARYTERMINAL | names: "A-Fixt_curve_" | property sets: Pset_SanitaryTerminalTypeCommon, EPset_Drawing
        1 x IFCDOOR | DOOR | names: "A-Door_curve_" | property sets: Pset_DoorCommon
        2 x IFCSTAIR | names: "A-Stairs_curve_" | property sets: Pset_StairCommon
        2 x IFCBUILDINGELEMENTPROXY | type IFCGEOGRAPHICELEMENTTYPE "car" | COMPLEX | names: "GeographicElement" | property sets: Pset_BuildingElementProxyCommon, OD_Options
        8 x IFCCOVERING | type IFCCOVERINGTYPE "Curb" | names: "Beam" | material: profiles ("6" RAMP CURB") | property sets: EPset_Parametric, OD_Options, Pset_BeamCommon, EPset_Drawing
        7 x IFCFOOTING | type IFCFOOTINGTYPE "DIAMOND PIER DP-75/50" | names: "Slab" | property sets: Pset_FootingCommon, EPset_Drawing
        7 x IFCCOLUMN | type IFCCOLUMNTYPE "6x6" | names: "Column" | material: profiles ("b") | property sets: EPset_Parametric, Pset_ColumnCommon
      IFCSPACE "110" | long name "STORAGE" | INTERNAL
      IFCSPACE "107" | long name "FITTING"
      IFCSPACE "105" | long name "STORAGE"
      IFCSPACE "102" | long name "CORRIDOR - BACK-OF-HOUSE"
      IFCSPACE "103" | long name "RESTROOM"
      IFCSPACE "108" | long name "FITTING"
      IFCSPACE "111" | long name "CORRIDOR" | INTERNAL
      IFCSPACE "101" | long name "REGISTER"
      IFCSPACE "104" | long name "STORAGE"
      IFCSPACE "106" | long name "DISPLAY AREA 2"
      IFCSPACE "109" | long name "STORAGE" | INTERNAL
      IFCSPACE "100" | long name "DISPLAY AREA 1" | INTERNAL
      IFCBUILDINGSTOREY "My Storey"
        contains 486 elements
          387 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Continuous Angle1:Continuous Angle:1463390", "Continuous Angle2:Continuous Angle:1578039", "Continuous Angle3:Continuous Angle:1578050" (+384 more) | material: "ACOUSTICAL SEALANT"; constituents "concrete" (); "TOP METAL STUD TRACK (FASTENER 24" O.C.)"; "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)"; "METAL RUNNER CHANNEL; FASTEN @ 24" O.C."; "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: EPset_Drawing, BBIM_Array
          1 x IFCDOOR | type IFCDOORTYPE "3070P" | names: "Door" | material: constituents "existing" ("DOOR & FRAME") | property sets: Pset_DoorCommon
          1 x IFCSLAB | type IFCSLABTYPE "FLR150" | names: "Slab" | material: layers ("GENERIC_FLOOR" 1.) | property sets: EPset_Parametric, Qto_SlabBaseQuantities, EPset_Drawing, Pset_SlabCommon
          1 x IFCDOOR | type IFCDOORTYPE "30"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "34"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "34"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "36"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "36"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "32"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "30"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          3 x IFCWALL | type IFCWALLTYPE "W1" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORTYPE "30"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: EPset_Drawing
          1 x IFCDOOR | type IFCDOORTYPE "34"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "32"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "34"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "36"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          1 x IFCDOOR | type IFCDOORTYPE "36"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna")
          30 x IFCBEAM | type IFCBEAMTYPE "2x12 JOIST" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, Pset_BeamCommon, BBIM_Array
          1 x IFCBEAM | type IFCBEAMTYPE "(3) 2x12 BEAM" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, Pset_BeamCommon
          2 x IFCBEAM | type IFCBEAMTYPE "(2) 2x10 BEAM" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, Pset_BeamCommon
          4 x IFCBEAM | type IFCBEAMTYPE "(2) 2x8 BEAM" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, Pset_BeamCommon
          14 x IFCBEAM | type IFCBEAMTYPE "2x8 JOIST" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, BBIM_Array, Pset_BeamCommon, EPset_Drawing
          10 x IFCBEAM | type IFCBEAMTYPE "2x6 JOIST" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, BBIM_Array, Pset_BeamCommon
          5 x IFCBEAM | type IFCBEAMTYPE "2x10 JOIST" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, BBIM_Array, Pset_BeamCommon
          2 x IFCBEAM | type IFCBEAMTYPE "TREATED 2x10 RIM JOIST" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, Pset_BeamCommon
          1 x IFCBEAM | type IFCBEAMTYPE "2x LEDGER" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, Pset_BeamCommon
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "(3) 2x4" | names: "Column", "(3) 2x4 2X COLUMN" | material: profiles ("b") | property sets: EPset_Parametric, Pset_ColumnCommon, EPset_Drawing
          8 x IFCSTAIRFLIGHT | STRAIGHT | names: "Plane" | property sets: BBIM_Stair, Pset_StairFlightCommon, BBIM_Array, EPset_Drawing
          1 x IFCBEAM | type IFCBEAMTYPE "2x12 OR 1 3/4 x 7 1/4LVL" | names: "Beam" | material: profiles ("b") | property sets: EPset_Parametric, Pset_BeamCommon
          1 x IFCDOOR | type IFCDOORTYPE "14"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: OD_Options

Types
  IFCWALLTYPE "M358BØD_EX" | STANDARD | 15 occurrences | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWINDOWTYPE "Empty" | WINDOW | 18 occurrences | material: profiles "existing" ("WINDOW")
  IFCPLATETYPE "Empty" | CURTAIN_PANEL | 4 occurrences | material: layers "existing" ("EXISTING STOREFRONT" 0.0416666679084301)
  IFCDOORTYPE "3070L-SF" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCDOORTYPE "3070R-SF" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCDOORTYPE "21070R" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing
  IFCFURNITURETYPE "Neufert Toilet with Cistern" | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Generic Medium Sink" | 1 occurrence | property sets: EPset_Drawing
  IFCDOORTYPE "21070L" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: BBIM_Door
  IFCDOORTYPE "34"84"L" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:34" x 84":154865, Door-Single-Panel:34" x 84":154865:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "3070R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: "DOOR" | property sets: BBIM_Door, EPset_Drawing, OD_DoorType_Hackjob | description "WOOD FLUSH W/ HM FRAME"
  IFCDOORTYPE "36"84"R" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Pset_DoorCommon
  IFCFURNITURETYPE "Neufert Medium Basin" | 1 occurrence | property sets: EPset_Drawing
  IFCWALLTYPE "M6BØD" | STANDARD | 2 occurrences | material: layers "existing" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.5, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_WallCommon | description "5/8 GYP - 6 METAL(BATT) - 5/8 GYP"
  IFCWALLTYPE "M358BØD_DEMO" | STANDARD | 5 occurrences | material: layers "demolish" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "W2" | STANDARD | 1 occurrence | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "W1" | STANDARD | 4 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCWALLTYPE "EX" | 3 occurrences | material: layers "existing" ("b" 0.416667014360428, "WINDOW" 0.416667014360428) | description "GENERIC EXTERIOR"
  IFCSANITARYTERMINALTYPE "ADA Grab Bars" | element type "GRAB_BARS" | USERDEFINED | 1 occurrence | property sets: EPset_Drawing
  IFCDOORTYPE "36"80"R" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:36" x 80":154902, Door-Single-Panel:36" x 80":154902:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "36"80"L" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:36" x 80":154902, Door-Single-Panel:36" x 80":154902:1, Pset_DoorCommon, EPset_Drawing
  IFCSLABTYPE "NEW ASPHALT DRIVE WAY" | 5 occurrences | material: layers "20Fill" ("ASPHALT DRIVEWAY" 0.984251976013184)
  IFCDOORTYPE "30"80"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCSLABTYPE "COMPOSITE DECK - HORZ." | FLOOR | 7 occurrences | material: layers "HorzLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric
  IFCSLABTYPE "COMPOSITE DECK - VERT." | FLOOR | 9 occurrences | material: layers "VertLines6in48scale" ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric
  IFCELECTRICAPPLIANCETYPE "Neufert Washing Machine" | 2 occurrences
  IFCSLABTYPE "CONCRETE SLAB" | FLOOR | 2 occurrences | material: layers "concrete" ("CONCRETE RAMP & LANDING" 0.5) | property sets: EPset_Parametric
  IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | 2 occurrences | property sets: EPset_Drawing
  IFCWALLTYPE "Basic Wall:W4BØD - (5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP)" | STANDARD | 9 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCDOORTYPE "24"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing
  IFCSANITARYTERMINALTYPE "Neufert Sink 124x44" | 2 occurrences
  IFCWALLTYPE "GENERIC 7"" | STANDARD | 1 occurrence | material: layers "poche" ("GENERIC POCHE" 0.583333313465118) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Core_Fill_8in" | COMPLEX | 10 occurrences | property sets: EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "Horz Ladder Reinforcing" | COMPLEX | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "8inCMU" | COMPLEX | 10 occurrences | property sets: EPset_Drawing
  IFCSLABTYPE "EXISTING DRIVEWAY" | 1 occurrence | material: layers "10Fill" ("EXISTING ASPHALT DRIVEWAY" 0.984251976013184)
  IFCSLABTYPE "FLR150" | 3 occurrences | material: layers ("GENERIC_FLOOR" 1.)
  IFCBUILDINGELEMENTPROXYTYPE "Morter_8inCMU" | COMPLEX | 11 occurrences
  IFCFURNITURETYPE "Neufert Retail 8-Seater Rectangular Table" | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Neufert Retail 6-Seater Circular Table" | 1 occurrence
  IFCGEOGRAPHICELEMENTTYPE "car" | 2 occurrences
  IFCCOVERINGTYPE "Curb" | 8 occurrences | material: profiles ("6" RAMP CURB")
  IFCFOOTINGTYPE "DIAMOND PIER DP-75/50" | 7 occurrences
  IFCCOLUMNTYPE "6x6" | 7 occurrences | material: profiles ("b")
  IFCDOORTYPE "3070P" | 1 occurrence | property sets: EPset_Drawing
  IFCDOORTYPE "30"80"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"80"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:34" x 80":154791, Door-Single-Panel:34" x 80":154791:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"84"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:34" x 84":154865, Door-Single-Panel:34" x 84":154865:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "32"84"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:32" x 84":154765, Door-Single-Panel:32" x 84":154765:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "30"84"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "30"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"80"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:34" x 80":154791, Door-Single-Panel:34" x 80":154791:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "32"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:32" x 84":154765, Door-Single-Panel:32" x 84":154765:1, Pset_DoorCommon
  IFCDOORTYPE "36"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Pset_DoorCommon
  IFCBEAMTYPE "2x12 JOIST" | BEAM | 30 occurrences | material: profiles ("b")
  IFCBEAMTYPE "(3) 2x12 BEAM" | BEAM | 1 occurrence | material: profiles ("b")
  IFCBEAMTYPE "(2) 2x10 BEAM" | BEAM | 2 occurrences | material: profiles ("b")
  IFCBEAMTYPE "(2) 2x8 BEAM" | BEAM | 4 occurrences | material: profiles ("b")
  IFCBEAMTYPE "2x8 JOIST" | BEAM | 14 occurrences | material: profiles ("b")
  IFCBEAMTYPE "2x6 JOIST" | BEAM | 10 occurrences | material: profiles ("b")
  IFCBEAMTYPE "2x10 JOIST" | BEAM | 5 occurrences | material: profiles ("b")
  IFCBEAMTYPE "TREATED 2x10 RIM JOIST" | BEAM | 2 occurrences | material: profiles ("b")
  IFCBEAMTYPE "2x LEDGER" | BEAM | 1 occurrence | material: profiles ("b")
  IFCCOLUMNTYPE "(3) 2x4" | 2 occurrences | material: profiles ("b")
  IFCBEAMTYPE "2x12 OR 1 3/4 x 7 1/4LVL" | BEAM | 1 occurrence | material: profiles ("b")
  IFCDOORTYPE "14"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing

Property sets
  EPset_Parametric | properties | on 105 objects (70 IFCBEAM, 18 IFCWINDOW, 9 IFCCOLUMN, 8 IFCCOVERING)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 40 objects (40 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 37 objects (27 IFCSLAB, 5 IFCFOOTING, 3 IFCPLATE, 1 IFCGEOGRAPHICELEMENT)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 3 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  Pset_DoorCommon | properties | on 10 objects (10 IFCDOOR)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    Status in {"NEW"} (IFCLABEL)
  Pset_DoorCommon | properties | on 3 objects (2 IFCDOOR, 1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_DoorCommon | properties | on 14 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 2.1946486495 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 2.19464874267578 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 22 objects (22 IFCWALL)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_WallCommon | properties | on 9 objects (9 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  Pset_WallCommon | properties | on 1 type object
    Status in {"EXISTING"} (IFCLABEL)
    ThermalTransmittance (no value)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 20.4724407196045 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 type object
    IsExternal = TRUE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
  EPset_Drawing | properties | on 76 objects (16 IFCANNOTATION, 10 IFCWALL, 8 IFCBUILDINGELEMENTPROXY, 8 IFCSLAB) | on 26 type objects
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
  EPset_Drawing | properties | on 3 objects (3 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "material.Category" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/4" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    Exclude = ".IfcElement[r"Pset_.*Common"."Status"="NEW"]" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3/8"=1'-0"" (IFCLABEL)
    ImperialPrecision = "1/4" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "r"Pset_.*Common", material, material.Category, IfcElement" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/32" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = TRUE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/96" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    Include = ".IfcElement[r"Pset_.*Common"."Status"="NEW"]" (IFCTEXT)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/48" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    Include = ".IfcElement[r"Pset_.*Common"."Status"="DEMOLISH"]" (IFCTEXT)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/48" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    Exclude = ".ifcSpace" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = TRUE (IFCBOOLEAN)
    HumanScale = "1"=30'" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/360" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing: 11 more contents on 11 objects not shown
  Pset_FurnitureTypeCommon | properties | on 5 objects (5 IFCFURNITURE)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 4 objects (4 IFCFURNITURE)
    Status in {"NEW"} (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Qto_DoorBaseQuantities | quantities | on 4 objects (4 IFCDOOR)
    Area = 2.614 [square foot (conversion based)]
    Height = 2.197 [foot (conversion based)]
    Perimeter = 6.375 [foot (conversion based)]
    Width = 0.991 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 3 objects (3 IFCDOOR)
    Area = 2.173 [square foot (conversion based)]
    Height = 2.134 [foot (conversion based)]
    Perimeter = 6.299 [foot (conversion based)]
    Width = 1.016 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 2.729 [square foot (conversion based)]
    Height = 2.197 [foot (conversion based)]
    Perimeter = 6.477 [foot (conversion based)]
    Width = 1.041 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 0. [square foot (conversion based)]
    Height = 0. [foot (conversion based)]
    Perimeter = 1.975 [foot (conversion based)]
    Width = 0.987 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 2.729 [square foot (conversion based)]
    Height = 84. [foot (conversion based)]
    Perimeter = 6.477 [foot (conversion based)]
    Width = 36. [foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 2 objects (2 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 47.424 [square foot (conversion based)]
    GrossFloorArea = 47.424 [square foot (conversion based)]
    GrossPerimeter = 28.217 [foot (conversion based)]
    GrossVolume = 466.767 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 47.424 [square foot (conversion based)]
    NetFloorArea = 47.424 [square foot (conversion based)]
    NetVolume = 466.767 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 99.597 [square foot (conversion based)]
    GrossFloorArea = 99.597 [square foot (conversion based)]
    GrossPerimeter = 40.374 [foot (conversion based)]
    GrossVolume = 980.287 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 99.597 [square foot (conversion based)]
    NetFloorArea = 99.597 [square foot (conversion based)]
    NetVolume = 980.287 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 34.309 [square foot (conversion based)]
    GrossFloorArea = 34.309 [square foot (conversion based)]
    GrossPerimeter = 23.447 [foot (conversion based)]
    GrossVolume = 337.685 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 34.309 [square foot (conversion based)]
    NetFloorArea = 34.309 [square foot (conversion based)]
    NetVolume = 337.685 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 10.609 [square foot (conversion based)]
    GrossFloorArea = 10.609 [square foot (conversion based)]
    GrossPerimeter = 13.656 [foot (conversion based)]
    GrossVolume = 104.423 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 10.609 [square foot (conversion based)]
    NetFloorArea = 10.609 [square foot (conversion based)]
    NetVolume = 104.423 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 103.345 [square foot (conversion based)]
    GrossFloorArea = 103.345 [square foot (conversion based)]
    GrossPerimeter = 48.665 [foot (conversion based)]
    GrossVolume = 1017.179 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 103.345 [square foot (conversion based)]
    NetFloorArea = 103.345 [square foot (conversion based)]
    NetVolume = 1017.179 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 44.285 [square foot (conversion based)]
    GrossFloorArea = 44.285 [square foot (conversion based)]
    GrossPerimeter = 26.671 [foot (conversion based)]
    GrossVolume = 435.875 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 44.285 [square foot (conversion based)]
    NetFloorArea = 44.285 [square foot (conversion based)]
    NetVolume = 435.875 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 140.281 [square foot (conversion based)]
    GrossFloorArea = 140.281 [square foot (conversion based)]
    GrossPerimeter = 73.518 [foot (conversion based)]
    GrossVolume = 1380.721 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 140.281 [square foot (conversion based)]
    NetFloorArea = 140.281 [square foot (conversion based)]
    NetVolume = 1380.721 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 130.76 [square foot (conversion based)]
    GrossFloorArea = 130.76 [square foot (conversion based)]
    GrossPerimeter = 45.749 [foot (conversion based)]
    GrossVolume = 1287.006 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 130.76 [square foot (conversion based)]
    NetFloorArea = 130.76 [square foot (conversion based)]
    NetVolume = 1287.006 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities: 3 more contents on 3 objects not shown
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 84. [foot (conversion based)]
    Width = 36. [foot (conversion based)]
  EPset_Annotation | properties | on 22 objects (22 IFCANNOTATION)
    Classes = "oblique" (IFCLABEL)
  EPset_Annotation | properties | on 10 objects (10 IFCANNOTATION)
    Classes = "fill-bg" (IFCLABEL)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.656 [foot (conversion based)]
    GrossArea = 1408.847 [square foot (conversion based)]
    GrossVolume = 924.44 [cubic foot (conversion based)]
    Length = 53.742 [foot (conversion based)]
    NetArea = 1408.847 [square foot (conversion based)]
    NetVolume = 924.44 [cubic foot (conversion based)]
    Perimeter = 160.338 [foot (conversion based)]
    Width = 26.427 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.072 [foot (conversion based)]
    GrossArea = 16.404 [square foot (conversion based)]
    GrossVolume = 1.181 [cubic foot (conversion based)]
    Length = 5. [foot (conversion based)]
    NetArea = 16.404 [square foot (conversion based)]
    NetVolume = 1.181 [cubic foot (conversion based)]
    Perimeter = 16.562 [foot (conversion based)]
    Width = 3.281 [foot (conversion based)]
  Pset_WindowCommon | properties | on 14 objects (14 IFCWINDOW)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_PlateCommon | properties | on 3 objects (3 IFCPLATE)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_SanitaryTerminalTypeCommon | properties | on 6 objects (6 IFCSANITARYTERMINAL)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_SanitaryTerminalTypeCommon | properties | on 6 objects (6 IFCSANITARYTERMINAL)
    Status in {"NEW"} (IFCLABEL)
  Pset_SanitaryTerminalTypeCommon | properties | on 1 object (1 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_SlabCommon | properties | on 15 objects (15 IFCSLAB)
    Status in {"NEW"} (IFCLABEL)
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    Status in {"NEW"} (IFCTEXT)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    Status in {"EXISTING"} (IFCLABEL)
  BBIM_reference_image_0 | properties | on 1 object (1 IFCBUILDING)
    Position X = "24.34749412536621" (IFCLABEL)
    Position Y = "-17.135032653808594" (IFCLABEL)
    Position Z = "0.0" (IFCLABEL)
    Rotation X = "0.0" (IFCLABEL)
    Rotation Y = "-0.0" (IFCLABEL)
    Rotation Z = "-3.1415929794311523" (IFCLABEL)
    Scale X = "-21.253463745117188" (IFCLABEL)
    Scale Y = "-21.253463745117188" (IFCLABEL)
    Scale Z = "-21.253463745117188" (IFCLABEL)
    image = "D:\Repositórios\OpeningDesign\mineral_point_residence\Existing Conditions and Code Research\Existing Conditions\aerial_2017.jpg" (IFCLABEL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    Status in {"NEW"} (IFCLABEL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    Status in {"EXISTING"} (IFCLABEL)
  OD_Options | properties | on 26 objects (7 IFCBUILDINGELEMENTPROXY, 6 IFCSLAB, 4 IFCWALL, 3 IFCSANITARYTERMINAL)
    OD_Option_1 = "" (IFCTEXT)
    OD_Option_2 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 22 objects (6 IFCCOVERING, 5 IFCWALL, 4 IFCSLAB, 3 IFCSANITARYTERMINAL)
    OD_Option_1 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
    OD_Options_2 = "" (IFCTEXT)
  OD_Options | properties | on 14 objects (10 IFCBUILDINGELEMENTPROXY, 1 IFCDOOR, 1 IFCRAILING, 1 IFCSLAB)
    OD_Option_1 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    OD_Option_1 = "" (IFCTEXT)
    OD_Option_2 = "" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 4 objects (2 IFCSLAB, 1 IFCBUILDINGELEMENTPROXY, 1 IFCDOOR)
    OD_Option_2 = "N" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 1 object (1 IFCSLAB)
    OD_Option_1 = "N" (IFCTEXT)
    OD_Option_2 = "" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  OD_Options | properties | on 1 object (1 IFCWALL)
    OD_Option_2 = "D" (IFCTEXT)
  OD_Options | properties | on 1 object (1 IFCSLAB)
    OD_Option_2 = "" (IFCTEXT)
    OD_Option_3 = "N" (IFCTEXT)
    OD_Option_4 = "N" (IFCTEXT)
  Pset_BeamCommon | properties | on 69 objects (69 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_BeamCommon | properties | on 8 objects (8 IFCCOVERING)
    Status in {"NEW"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 20 objects (20 IFCBUILDINGELEMENTPROXY)
    Status in {"NEW"} (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Status in {"NEW"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_ElectricApplianceTypeCommon | properties | on 2 objects (2 IFCELECTRICAPPLIANCE)
    Status in {"NEW"} (IFCLABEL)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Status in {"NEW"} (IFCLABEL)
  BBIM_Array | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3iGRJZfy51iAd8K3LgiYDq" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0zDYnHKt9D9xBQ0J7EbG8P" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0QwQTUhPr6EAqfEjNat8se" (IFCLABEL)
  BBIM_Array | properties | on 8 objects (8 IFCBEAM)
    Data (no value)
    Parent = "0kmier3oX7JhM8LuwAfC20" (IFCLABEL)
  BBIM_Array | properties | on 7 objects (7 IFCBEAM)
    Data (no value)
    Parent = "3iyTQJUIj2$hgC$6tqQaUh" (IFCLABEL)
  BBIM_Array | properties | on 6 objects (6 IFCBEAM)
    Data (no value)
    Parent = "1fQHr_THPBMRqY0nWZRTxz" (IFCLABEL)
  BBIM_Array | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3QecqJiErB$9TeAgOjclzW" (IFCLABEL)
  BBIM_Array | properties | on 4 objects (4 IFCBEAM)
    Data (no value)
    Parent = "3BnObHYRj3kQZ3rq58RDjW" (IFCLABEL)
  BBIM_Array: 22 more contents on 36 objects not shown
  BBIM_Stair | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Data = "{"stair_type": "CONCRETE", "width": 0.12500000154487104, "height": 2.4791699381950956, "number_of_treads": 3, "tread_run": 0.8334010213691732, "base_slab_depth": 0.32020996757379666, "top_slab_depth": 0.25000002753390416, "has_top_nib": false, "tread_depth": 0.44947509651421874}" (IFCLABEL)
  BBIM_Stair | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    Data = "{"stair_type": "CONCRETE", "width": 0.12500000154487104, "height": 2.0624001038668975, "number_of_treads": 3, "tread_run": 1.5002499845397128, "base_slab_depth": 0.32020996757379666, "top_slab_depth": 0.25000002753390416, "has_top_nib": false, "tread_depth": 0.44947509651421874}" (IFCLABEL)
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NumberOfRiser = 4. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    RiserHeight = 0.619792461395264 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Status in {"NEW"} (IFCLABEL)
    TreadLength = 0.449475109577179 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_StairFlightCommon | properties | on 4 objects (4 IFCSTAIRFLIGHT)
    NumberOfRiser = 4. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    RiserHeight = 0.515600025653839 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Status in {"NEW"} (IFCLABEL)
    TreadLength = 0.449475109577179 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_ColumnCommon | properties | on 7 objects (7 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
  Pset_FootingCommon | properties | on 7 objects (7 IFCFOOTING)
    LoadBearing = TRUE (IFCBOOLEAN)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 7.0, "overall_width": 3.3333332538604736, "lining_properties": {"lining_depth": 0.3333333432674408, "lining_thickness": 0.1666666716337204, "lining_offset": 0.32999998331069946, "lining_to_panel_offset_x": 0.1666666716337204, "lining_to_panel_offset_y": 0.08202099800109863, "transom_thickness": 0.0, "threshold_thickness": 0.08202099800109863, "threshold_depth": 0.32808399200439453, "threshold_offset": 0.32999998331069946}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0, "overall_width": 3.3333332538604736, "lining_properties": {"lining_depth": 0.3333333432674408, "lining_thickness": 0.1666666716337204, "lining_offset": 0.3333333432674408, "lining_to_panel_offset_x": 0.1666666716337204, "lining_to_panel_offset_y": 0.08202099800109863, "transom_thickness": 0.0, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0625, "overall_width": 2.958329916000366, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 7.0625, "overall_width": 2.958329916000366, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_RIGHT", "overall_height": 7.0625, "overall_width": 3.125, "lining_properties": {"lining_depth": 0.4059999883174896, "lining_thickness": 0.0625, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.0625, "lining_to_panel_offset_y": 0.0625, "transom_thickness": 0.0, "casing_thickness": 0.20833300054073334, "casing_depth": 0.04166699945926666, "threshold_thickness": 0.0}, "panel_properties": {"panel_depth": 0.1148293986916542, "panel_width_ratio": 1.0}}" (IFCLABEL)
  Door-Single-Panel:34" x 84":154865 | predefined | on 2 type objects
  Door-Single-Panel:34" x 84":154865:1 | predefined | on 2 type objects
  OD_DoorType_Hackjob | properties | on 1 type object
    DoorHeight = "7' - 0"" (IFCTEXT)
    DoorWidth = "3' - 0"" (IFCTEXT)
    TypeComments = "MATCH EXISTING (HEIGHT, MATERIAL/FINISH, HARDWARE)" (IFCTEXT)
  Door-Single-Panel:36" x 84":154924 | predefined | on 2 type objects
  Door-Single-Panel:36" x 84":154924:1 | predefined | on 2 type objects
  Door-Single-Panel:36" x 80":154902 | predefined | on 2 type objects
  Door-Single-Panel:36" x 80":154902:1 | predefined | on 2 type objects
  Door-Single-Panel:30" x 80":154643 | predefined | on 2 type objects
  Door-Single-Panel:30" x 80":154643:1 | predefined | on 2 type objects
  Pset_ElementShading | properties | on 2 type objects
    Roughness = 1. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_ProductRequirements | properties | on 2 type objects
    Category = "Walls" (IFCLABEL)
  Door-Single-Panel:30" x 84":154723 | predefined | on 4 type objects
  Door-Single-Panel:30" x 84":154723:1 | predefined | on 4 type objects
  Door-Single-Panel:34" x 80":154791 | predefined | on 2 type objects
  Door-Single-Panel:34" x 80":154791:1 | predefined | on 2 type objects
  Door-Single-Panel:32" x 84":154765 | predefined | on 2 type objects
  Door-Single-Panel:32" x 84":154765:1 | predefined | on 2 type objects