IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "ExchangeRequirement [Any]"
File name: "IFC Hero Model.ifc"
Time stamp: "2025-08-06T11:11:18"
Author: "JLaukal"
Organization: "Trimble Inc."
Preprocessor: "TrimBimToIFC rel. 4.0.2"
Originating system: "Trimble Inc. - SketchUp - 2025.0"
Authorization: "IFC4 model"
Application: "Trimble Inc. - SketchUp - 2025.0" version "2025.0" identifier "SketchUp" by Organization "Trimble Inc."

People and organizations
  Person "Unknown" id "JLaukal" of Organization "Trimble Inc."
  Owner history of Person "Unknown" id "JLaukal" of Organization "Trimble Inc." | application "Trimble Inc. - SketchUp - 2025.0" version "2025.0" identifier "SketchUp" by Organization "Trimble Inc." | change NOCHANGE | created 1754467200 (2025-08-06T08:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN

Spatial structure
IFCPROJECT "Mies Van der Rohe"
  IFCSITE "Sants Montjuic" | elevation above sea level 0.
    IFCBUILDING "Pavillon de Barcelona"
      IFCBUILDINGSTOREY "Foundation"
        contains 11 elements
          1 x IFCSLAB | FLOOR | names: "Slab Foundation" | material: "Travertine" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_SlabCommon
          3 x IFCCOVERING | FLOORING | names: "Water Stones Small", "Water Stones Big", "Water Covering Base" | material: "RiverRock4inch"; "GreenMarble" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_CoveringCommon
          4 x IFCCOVERING | CLADDING | names: "Water Covering Front", "Water Covering Back", "Water Covering Left" (+1 more) | material: "GreenMarble" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_CoveringCommon
          2 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Water_Statue", "Water_Entrance" | material: "BlueGlass"; "Water" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_BuildingElementProxyCommon
          1 x IFCSTAIR | STRAIGHT_RUN_STAIR | names: "Access Stair" | material: "Travertine" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_StairCommon
      IFCBUILDINGSTOREY "Roof"
        contains 7 elements
          4 x IFCROOF | FLAT_ROOF | names: "Roof Office Base", "Roof Main Base", "Roof Top Office" (+1 more) | material: "*9"; "WhitePainting_Snow" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_RoofCommon
          2 x IFCCOVERING | ROOFING | names: "Roof Office Covering", "Roof Main Covering" | material: "Stainless steel" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_CoveringCommon
          1 x IFCWINDOW | SKYLIGHT | names: "Skylight" | material: "BPV_M01B" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_WindowCommon
      IFCBUILDINGSTOREY "First Floor"
        contains 30 elements
          8 x IFCCOLUMN | PILASTER | names: "Stainless Steel Column" | material: "Stainless steel" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_ColumnCommon
          6 x IFCWALL | PARTITIONING | names: "Wall Travertine#3", "Wall Green Marble", "Wall Travertine#1" (+3 more) | material: "Travertine"; "GreenMarble"; "GoldenOnixMarble"; "GreenAlpineMarble" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Water_Skylight" | material: "BlueGlass" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_BuildingElementProxyCommon
          5 x IFCFURNITURE | CHAIR | names: "Barcelona Chair", "Barcelona Chair with Backrest", "Alba" | material: "[Color D01]"; "*" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | object type "Carpet" | USERDEFINED | names: "Carpet" | material: "Carpet_04_1K" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | names: "Marble Bench" | material: "Travertine" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_FurnitureTypeCommon
          8 x IFCCURTAINWALL | names: "Curtain Wall Front", "Curtain Wall Division Office", "Curtain Wall Shading" (+4 more) | material: "Stainless steel" | property sets: SU_InstanceSet, SU_DefinitionSet, Pset_CurtainWallCommon

Property sets
  SU_InstanceSet | properties | on 54 objects (9 IFCCOVERING, 8 IFCCOLUMN, 8 IFCCURTAINWALL, 7 IFCFURNITURE)
    Owner = "" (IFCTEXT)
    Status = "" (IFCTEXT)
  SU_DefinitionSet | properties | on 54 objects (9 IFCCOVERING, 8 IFCCOLUMN, 8 IFCCURTAINWALL, 7 IFCFURNITURE)
    Price = "" (IFCTEXT)
    Size = "" (IFCTEXT)
    Url = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = TRUE (IFCLOGICAL)
    EntranceLevel = FALSE (IFCBOOLEAN)
    GrossPlannedArea = 1320. (IFCAREAMEASURE) [SQUARE_METRE]
    LoadBearingCapacity = 0. (IFCPLANARFORCEMEASURE)
    NetPlannedArea = 900. (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Foundation" (IFCIDENTIFIER)
    SprinklerProtection = FALSE (IFCBOOLEAN)
    SprinklerProtectionAutomatic = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = TRUE (IFCLOGICAL)
    EntranceLevel = FALSE (IFCBOOLEAN)
    GrossPlannedArea = 393. (IFCAREAMEASURE) [SQUARE_METRE]
    LoadBearingCapacity = 0. (IFCPLANARFORCEMEASURE)
    NetPlannedArea = 393. (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Roof" (IFCIDENTIFIER)
    SprinklerProtection = FALSE (IFCBOOLEAN)
    SprinklerProtectionAutomatic = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = TRUE (IFCLOGICAL)
    EntranceLevel = FALSE (IFCBOOLEAN)
    GrossPlannedArea = 1320. (IFCAREAMEASURE) [SQUARE_METRE]
    LoadBearingCapacity = 0. (IFCPLANARFORCEMEASURE)
    NetPlannedArea = 900. (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "FirstFloor" (IFCIDENTIFIER)
    SprinklerProtection = FALSE (IFCBOOLEAN)
    SprinklerProtectionAutomatic = FALSE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "55" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "120" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Reference = "Slab-001" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Stones" (IFCTEXT)
    FireRating = "120" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-006" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Green Marble" (IFCTEXT)
    FireRating = "120" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-003" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Green Marble" (IFCTEXT)
    FireRating = "120" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-001" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Green Marble" (IFCTEXT)
    FireRating = "120" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-004" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Green Marble" (IFCTEXT)
    FireRating = "120" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-005" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Green Marble" (IFCTEXT)
    FireRating = "120" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-002" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Stateless Metal" (IFCTEXT)
    FireRating = "30" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-007" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    AcousticRating = "50" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Stateless Metal" (IFCTEXT)
    FireRating = "30" (IFCLABEL)
    FlammabilityRating = "Non-combustible" (IFCLABEL)
    FragilityRating = "Low" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Covering-006" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    FireRating = "120" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Proxy-002" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    FireRating = "120" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Proxy-001" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 2.5 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    FireRating = "0" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Proxy-003" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 0.1 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireExit (no value)
    FireRating (no value)
    HandicapAccessible (no value)
    HasNonSkidSurface (no value)
    IsExternal (no value)
    LoadBearing (no value)
    NosingLength (no value)
    NumberOfRiser (no value)
    NumberOfTreads (no value)
    Reference (no value)
    RequiredHeadroom (no value)
    RiserHeight (no value)
    Status = "" (IFCTEXT)
    ThermalTransmittance (no value)
    TreadLength (no value)
    TreadLengthAtInnerSide (no value)
    TreadLengthAtOffset (no value)
    WaistThickness (no value)
    WalkingLineOffset (no value)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    AcousticRating = "50" (IFCLABEL)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Roof-003" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 0.18 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    AcousticRating = "50" (IFCLABEL)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Roof-001" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 0.18 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    AcousticRating = "50" (IFCLABEL)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Roof-004" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 0.18 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    AcousticRating = "50" (IFCLABEL)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Roof-002" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 0.18 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "38" (IFCLABEL)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "30" (IFCLABEL)
    GlazingAreaFraction = 0.75 (IFCPOSITIVERATIOMEASURE)
    HasDrive = FALSE (IFCBOOLEAN)
    HasSillExternal = FALSE (IFCBOOLEAN)
    HasSillInternal = FALSE (IFCBOOLEAN)
    Infiltration = 0.1 (IFCVOLUMETRICFLOWRATEMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    MechanicalLoadRating = "Medium" (IFCLABEL)
    Reference = "Window-001" (IFCIDENTIFIER)
    SecurityRating = "RC3" (IFCLABEL)
    SmokeStop = FALSE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 1.4 (IFCTHERMALTRANSMITTANCEMEASURE)
    WaterTightnessRating = "Class 9A" (IFCLABEL)
    WindLoadRating = "2000" (IFCLABEL)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    FireRating = "90" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Column-001" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
    ThermalTransmittance = 2.2 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    AcousticRating = "45" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-006" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 0.35 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    AcousticRating = "45" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-003" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 0.35 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    AcousticRating = "45" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-004" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 0.35 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    AcousticRating = "45" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-001" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 0.35 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    AcousticRating = "45" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-002" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 0.35 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    AcousticRating = "45" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    FireRating = "90" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-005" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 0.35 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_FurnitureTypeCommon | properties | on 2 objects (2 IFCFURNITURE)
    Description = "Barcelona Chair" (IFCLABEL)
    IsBuiltIn = FALSE (IFCBOOLEAN)
    MainColor = "White" (IFCLABEL)
    NominalDepth = 600. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = 450. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 600. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Style = "Modernist" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 2 objects (2 IFCFURNITURE)
    Description = "Barcelona Chair" (IFCLABEL)
    IsBuiltIn = FALSE (IFCBOOLEAN)
    MainColor = "White" (IFCLABEL)
    NominalDepth = 750. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = 1050. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 750. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Style = "Modernist" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCFURNITURE)
    Description = "Carpet" (IFCLABEL)
    IsBuiltIn = FALSE (IFCBOOLEAN)
    MainColor = "Blue" (IFCLABEL)
    NominalDepth = 415. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = 10. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 615. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Style = "Modernist" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCFURNITURE)
    Description = "Stone Bench" (IFCLABEL)
    IsBuiltIn = FALSE (IFCBOOLEAN)
    MainColor = "Beige" (IFCLABEL)
    NominalDepth = 700. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = 600. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 15000. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Style = "Modernist" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 1 object (1 IFCFURNITURE)
    Description = "Alba Statue" (IFCLABEL)
    IsBuiltIn = FALSE (IFCBOOLEAN)
    MainColor = "Gray" (IFCLABEL)
    NominalDepth = 900. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = 32000. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 900. (IFCPOSITIVELENGTHMEASURE) [METRE]
    Style = "Modernist" (IFCLABEL)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    AcousticRating = "40" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CurtainWall-006" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 1.6 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    AcousticRating = "40" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CurtainWall-001" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 1.6 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    AcousticRating = "40" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CurtainWall-003" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 1.6 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    AcousticRating = "40" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CurtainWall-002" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 1.6 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    AcousticRating = "40" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CurtainWall-004" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 1.6 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    AcousticRating = "40" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    FireRating = "60" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "CurtainWall-005" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
    SurfaceSpreadOfFlame = "Class 0" (IFCLABEL)
    ThermalTransmittance = 1.6 (IFCTHERMALTRANSMITTANCEMEASURE)