IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "model.ifc"
Time stamp: "2023-11-12T19:03:26+00:00"
Preprocessor: "IfcOpenShell 0.7.0"
Originating system: "BlenderBIM 0.0.999999"
Authorization: "Nobody"

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "Ground Floor"
        contains 32 elements
          4 x IFCWALL | type IFCWALLTYPE "External wall" | names: "Wall" | material: layers ("Unknown" 0.100000001490116, "Unknown" 0.0750000029802322, "Unknown" 0.100000001490116) | property sets: EPset_Parametric
          4 x IFCWALL | type IFCWALLTYPE "Partition" | names: "Wall" | material: layers ("Unknown" 0.100000001490116) | property sets: EPset_Parametric
          4 x IFCDOOR | type IFCDOORTYPE "internal" | names: "Door"
          1 x IFCDOOR | type IFCDOORTYPE "internal" | SINGLE_SWING_LEFT | names: "Door"
          1 x IFCWINDOW | type IFCWINDOWTYPE "kitchen" | DOUBLE_PANEL_VERTICAL | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "lounge" | DOUBLE_PANEL_HORIZONTAL | names: "Window"
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Neufert Washing Machine" | names: "ElectricAppliance"
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Neufert Drier" | names: "ElectricAppliance" | property sets: EPset_Drawing
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Double bed" | names: "Furniture"
          3 x IFCFURNITURE | type IFCFURNITURETYPE "Generic Small Bedside Table" | names: "Furniture"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Residential 4-Seater Rectangular Table" | names: "Furniture"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Generic 3-Seater Sofa" | names: "Furniture"
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | names: "SanitaryTerminal"
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Shower 75x90" | names: "SanitaryTerminal"
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Medium Basin" | names: "SanitaryTerminal"
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Single Person Wardrobe" | names: "Furniture"
          1 x IFCWINDOW | type IFCWINDOWTYPE "bathroom" | DOUBLE_PANEL_HORIZONTAL | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "bedroom1" | TRIPLE_PANEL_VERTICAL | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "bedroom1" | names: "Window"
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Neufert Cooktop 58x51" | names: "ElectricAppliance"
      IFCBUILDINGSTOREY "Attic"
        contains 4 elements
          4 x IFCWALL | type IFCWALLTYPE "External wall" | names: "Wall" | material: layers ("Unknown" 0.100000001490116, "Unknown" 0.0750000029802322, "Unknown" 0.100000001490116) | property sets: EPset_Parametric

Types
  IFCWALLTYPE "External wall" | STANDARD | 8 occurrences | material: layers ("Unknown" 0.100000001490116, "Unknown" 0.0750000029802322, "Unknown" 0.100000001490116) | property sets: EPset_Parametric
  IFCWALLTYPE "Partition" | PARTITIONING | 4 occurrences | material: layers ("Unknown" 0.100000001490116) | property sets: EPset_Parametric
  IFCDOORTYPE "internal" | DOOR | SINGLE_SWING_LEFT | 5 occurrences | property sets: BBIM_Door
  IFCWINDOWTYPE "kitchen" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCWINDOWTYPE "lounge" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCELECTRICAPPLIANCETYPE "Neufert Washing Machine" | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "Neufert Drier" | 1 occurrence
  IFCFURNITURETYPE "Double bed" | 2 occurrences
  IFCFURNITURETYPE "Generic Small Bedside Table" | 3 occurrences
  IFCFURNITURETYPE "Neufert Residential 4-Seater Rectangular Table" | 1 occurrence
  IFCFURNITURETYPE "Generic 3-Seater Sofa" | 1 occurrence
  IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | 1 occurrence
  IFCSANITARYTERMINALTYPE "Neufert Shower 75x90" | 1 occurrence
  IFCSANITARYTERMINALTYPE "Neufert Medium Basin" | 1 occurrence
  IFCFURNITURETYPE "Neufert Single Person Wardrobe" | 1 occurrence
  IFCWINDOWTYPE "bathroom" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCWINDOWTYPE "bedroom1" | WINDOW | SINGLE_PANEL | 2 occurrences | property sets: BBIM_Window
  IFCELECTRICAPPLIANCETYPE "Neufert Cooktop 58x51" | 1 occurrence

Property sets
  EPset_Parametric | properties | on 12 objects (12 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS2" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:20" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/20" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCELECTRICAPPLIANCE)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 1.9500000476837158, "overall_width": 0.7620000243186951, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.0, "casing_thickness": 0.07500000298023224, "casing_depth": 0.004999999888241291, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 0.8999999761581421, "overall_width": 0.8999999761581421, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.05000000074505806, "first_mullion_offset": 0.44999998807907104}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 1.2000000476837158, "overall_width": 1.0, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.05000000074505806, "first_transom_offset": 0.800000011920929}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 0.8999999761581421, "overall_width": 0.7599999904632568, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.05000000074505806, "first_transom_offset": 0.6000000238418579}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_VERTICAL", "overall_height": 1.2000000476837158, "overall_width": 2.1500000953674316, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.05000000074505806, "first_mullion_offset": 0.75, "second_mullion_offset": 1.4500000476837158}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCTEXT)