IFC building model
Schema: "IFC4"
Description: "ViewDefinition [notYetAssigned]"
File name: "ifcwallelementedcase.ifc"
Time stamp: "2015-03-13T19:19:38"
Preprocessor: "Constructivity 0.9.8.2"
Originating system: "Constructivity 0.9.8.2"

Units
  AREAUNIT: square inch (conversion based)
  FORCEUNIT: pound-force (conversion based)
  LENGTHUNIT: inch (conversion based)
  MASSUNIT: pound (conversion based)
  PLANEANGLEUNIT: degree (conversion based)
  PRESSUREUNIT: pound-force per square inch (conversion based)
  THERMODYNAMICTEMPERATUREUNIT: Fahrenheit (conversion based)
  VOLUMEUNIT: cubic inch (conversion based)
  CURRENCY: USD

Spatial structure
IFCPROJECT "Project"
  IFCSITE "Site #1"
    contains 1 element
      1 x IFCWALLELEMENTEDCASE | type IFCWALLTYPE "Wood Framed Wall" | MOVABLE | names: "Wall #1" | parts: 2 IFCBUILDINGELEMENTPART, 1 IFCELEMENTASSEMBLY | material: layers "Wall" ((no material) 0.5, (no material) 3.5, (no material) 0.5)
IFCELEMENTASSEMBLYTYPE "Wood Stud Frame"
  IFCMEMBER "Track" | PLATE
  IFCMEMBER "Studs" | STUD
IFCWALLTYPE "Wood Framed Wall"
  IFCBUILDINGELEMENTPART "Panel Forward" | PRECASTPANEL
  IFCELEMENTASSEMBLY "Frame" | BRACED_FRAME
    IFCMEMBER "Track" | PLATE
    IFCMEMBER "Studs" | STUD
  IFCBUILDINGELEMENTPART "Panel Reverse" | PRECASTPANEL

Types
  IFCWALLTYPE "Wood Framed Wall" | 1 occurrence | material: layers "Wall" ((no material) 0.5, (no material) 3.5, (no material) 0.5)